Declaration of Conformity (DoC)


We,Shenzhen DOKE Electronic Co.,Ltd.
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China.

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s): Product Type:	Mobile Phone
Trademark：	Blackview
Model Number(s):	BV4800 Pro

(Name of product, type or model, batch or serial number) System components:
PIFA Antenna:BT/Wi-Fi2.4G:0.66dBi; WIFI5G:0.62dBi;
GSM900:-2.85dBi/DCS1800:0.91dBi; WCDMABandⅠ: 0.21dBi,BandⅧ:-2.96dBi; LTE: B1: 0.68dBi; B3: 0.88dBi; B7: 0.95dBi; B8: -2.76dBi;
B20: -3.26dBi; B28: -3.26dBi; B40: 0.21dBi; B41: 0.21dBi;


Adapter :
Model: HJ-0502000-EU
Input: 100-240V~50/60Hz 0.3A Output: 5.0V 2.0A 10.0W
Manufacturer: Shenzhen Huajin Electronics Co.,Ltd


RechargeableLi-ionBattery:
Model:LiU516386PHTT; Specification: DC 3.85V, 5180mAh, 19.94Wh; Manufacturer:Shenzhen Huatiantong Technology Co.,Ltd.

The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

HEALTH & SAFETY (Art. 3(1)(a)):

EN 50360:2017;

EN 50566:2017;

EN 62209-1:2016;

EN 62209-2:2010;

EN 62479:2010

EN IEC 62368-1:2020+A11:2020

EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)

ETSI EN 301 489-3 V2.1.1 (2019-03)

ETSI EN 301 489-17 V3.2.4 (2020-09)

ETSI EN 301 489-19 V2.2.1 (2022-09)

ETSI EN 301 489-52 V1.2.1 (2021-11) EN 55032:2015+A1:2020
EN 55035:2017+A11:2020

EN IEC 61000-3-2:2019+A1:2021 EN 61000-3-3:2013+A2:2021
Radio Spectrum (Article 3.2):

EN 301 511 V12.5.1 (2017-03);

EN 301 908-1 V15.1.1 (2021-09);

EN 301 908-2 V13.1.1 (2020-06);

EN 301 908-13 V13.2.1 (2022-02);

EN 300 328 V2.2.2 (2019-07);

EN 301 893 V2.1.1 (2017-05);

EN 300 330 V2.1.1 (2017-02)

EN 300 440 V2.2.1 (2018-07);

EN 303 413 V1.2.1 (2021-04);

EN 303 345-1 V1.1.1 (2019-06);

EN 303 345-3 V1.1.1 (2021-06);

Notified Body Involved:


Notified Body Name: Eurofins Electrical and Electronic Testing NA, Inc. Notified Body Number: 0980
Notified Body Assessment Performed: Module B/C on Article 3.1a, 3.1b, 3.2
EU-type examination certificate number: 3443-09-2024-240693 

RF Specification:


	
Function
	
Operation Frequency
	Max RF

outputpower:

	BLE
	2402MHz–2480MHz
	2.17dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	6.37dBm

	WIFI 802.11b/g/

n(HT20/40)
	802.11b/g/n(20MHz): 2412~2472MHz;

802.11n(40MHz):2422~2462MHz
	
15.83dBm

	Wi-Fi 5.2G(802.11a/n20/n4
0/ac20/ac40/ac80)
	802.11a/ n20/ac20:5180MHz~5240MHz

802.11 n40/ac40:5190MHz~5230MHz

802.11 ac80:5210MHz
	

12.96dBm

	Wi-Fi 5.8G(802.11a/n20/n4
0/ac20/ac40/ac80)
	802.11a/ n20/ac20:5745MHz~5825MHz

802.11 n40/ac40:5755MHz~5795MHz

802.11ac80:5775MHz
	

11.72dBm

	GSM/GPRS/EGPRS

900
	TX(Uplink):880M‐915MHZ;
RX(Downlink):925M‐960MHZ
	
31.62dBm

	GSM/GPRS/EGPRS

1800
	TX(Uplink):1710M‐1785MHZ;
RX(Downlink):1805M‐1880MHZ
	
28.76dBm

	
WCDMA B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
21.94dBm

	
WCDMA B8
	TX(Uplink): 880-915MHz;

RX(Downlink):925-960MHz
	
22.38dBm

	
LTE FDD B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
23.67dBm

	
LTE FDD B3
	TX(Uplink) :1710-1785MHz;

RX(Downlink):1805-1880MHz
	
23.5dBm

	
LTE FDD B7
	TX(Uplink) :2500-2570MHz;

RX(Downlink):2620-2690MHz
	
23.32dBm

	
LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz

RX(Downlink): 925 MHz to 960 MHz
	
24.29dBm

	
LTE FDD B20
	TX(Uplink): 832MHz~862MHz;

RX(Downlink): 791MHz~821MHz
	
23.71dBm

	
LTE FDD B28
	TX(Uplink): 703MHz~736MHz;

RX(Downlink): 758MHz~791MHz
	
23.65dBm

	
LTE TDD B40
	TX(Uplink)& RX(Downlink)

2300 MHz to 2400 MHz
	
23.27dBm

	
LTE TDD B41
	TX(Uplink)& RX(Downlink)

2496 MHz to 2690 MHz
	
23.65dBm

	NFC
	13.56MHz
	-3.56 dBuA/m@10m

	FM
	Rx: 87.5MHz~108MHz
	--

	GPS
	Rx: 1.57542GHz
	--
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)Tests for SAR are conducted using standard operating positions with the device transmitting at its highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used close to the body (at a minimum distance of 5mm/0mm) are:








Technical file held by:Shenzhen DOKE Electronic Co., Ltd

801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China.


Signed for and on behalf of: Shenzhen DOKE Electronic Co., Ltd

	Name and Title:
	zhang.liuwei/Manager

	Address:
	801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming

District, Shenzhen, China.






Signature of Authorized Person
2024-09-18
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