
Declaration of Conformity (DoC)


We, Shenzhen Gotron Electronic CO.,LTD.
7B01, Building A, Block 1, Anhongji Tianyao Plaza, Longhua District, Shenzhen City, Guangdong Province China
Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Smart Phone

	Trademark：
	ulefone

	Model Number(s):
	GQ5013TF, Armor 30, Armor 30 Ultra, Armor 30T Ultra, Armor 30T Pro, Armor 30 Lite, Armor 30s, Armor 30s Pro




System components:

PIFA Antenna: BT/Wi-Fi2.4G: -0.6 dBi; WIFI5.2G: 1.5 dBi; WIFI5.8G: 0.3 dBi
GSM900: -2.1dBi   PCS1800: -0.74dBi; WCDMA Band I: 0.8 dBi WCDMA Band VIII: -2.1 dBi;

LTE: Band 1: 0.8 dBi, Band 3: -0.74 dBi, Band 7: -0.35 dBi, Band 8: -2.1 dBi, Band 20: -3.4 dBi, Band 28: -4.4 dBi, 
Band 40: -4.38 dBi;

NFC: Loop Antenna
GPS: PIFA antenna

Adapter:
Model: HJ-PD66W-EU
Input: 100-240V AC50/60Hz 1.5A
Output: 5.0V⎓3.0A or 9.0V⎓3.0A or 12.0V⎓3.0A
or 15.0V⎓3.0A or 20.0V⎓3.25A or 11.0V⎓6.0A 66W MAX

Manufacturer of the adapter: Guangdong Quanzhi Technology Co.,Ltd.

Rechargeable Li-ion Battery:
Model: 5013; Specification: DC 3.87V, 12800mAh, 49.536Wh 
Manufacturer of battery: Shenzhen Huatiantong Technology Co., Ltd.
USB Cable: 100cm;

[image: C:\Users\admin\AppData\Local\Temp\QQ_1749721170213.png]



The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: 
Radio Equipment Directive RED (2014/53/EU)
The following harmonized standards and technical specifications have been applied:

Health & Safety (Article 3(1)(a)):

EN IEC 62368-1:2020+A11:2020
EN 50360:2017+A1:2023
EN 50566:2017+A1:2023
EN62209-1:2016
EN 62209-2:2010+A1:2019
EN 50663:2017
EN 62479: 2010

EMC (Article 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)
ETSI EN 301 489-3 V2.3.2 (2023-01)
ETSI EN 301 489-17 V3.2.4 (2020-09)
ETSI EN 301 489-19 V2.1.1 (2019-04)
ETSI EN 301 489-52 V1.2.1 (2021-11)
EN 55032:2015+A11:2020
EN 55035:2017+A11:2020
EN IEC 61000-3-2:2019+A1:2021
EN 61000-3-3:2013/A2:2021/AC:2022-01

Radio Spectrum (Article 3.2):

ETSI EN 300 328 V2.2.2 (2019-07)
ETSI EN 301 893 V2.1.1 (2017-05)
ETSI EN 300 440 V2.2.1 (2018-07)
ETSI EN 301 511 V12.5.1(2017-03)
ETSI EN 301 908-1 V15.2.1(2023-01)
ETSI EN 301 908-2 V13.1.1(2020-06)
ETSI EN 301 908-13 V13.2.1(2022-02)
ETSI EN 300 330 V2.1.1 (2017-02)
ETSI EN 303 345-1 V1.1.1 (2019-06)
ETSI EN 303 345-3 V1.1.1 (2021-06)
ETSI EN 303 413 V1.2.1 (2021-04)

Notified Body Involved:
	[bookmark: OLE_LINK27]Notified Body: 
	Intertek Semko AB 

	Notified Body Number: 
	0413

	Notified Body Assessment Performed: 
	Module B+C on Article 3.1a, 3.1b, 3.2

	EU-Type Examination Certificate Number: 
	[bookmark: _GoBack]SE-RED-2500527 Ed.1



RF Specification:

	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	2.04 dBm EIRP

	BT(BR+EDR)
	2402MHz–2480MHz
	3.72 dBm EIRP

	802.11b/g/n (HT20/40)
	802.11b/g/n (20MHz): 2412~2472MHz;

802.11n (40MHz):2422~2462MHz
	
15.73 dBm EIRP

	Wi-Fi 5.2G(802.11a/n20/n40/ac 20/ac40/ac80)

	
802.11a/ n20/ac20:5180MHz~5240MHz

802.11 n40/ac40:5190MHz~5230MHz

802.11 ac80:5210MHz
	


13.38 dBm EIRP

	Wi-Fi 5.8G(802.11a/n20/n40/ac 20/ac40/ac80)
	
802.11a/ n20/ac20:5745MHz~5825MHz

802.11 n40/ac40:5755MHz~5795MHz

802.11 ac80:57750MHz
	


11.98 dBm EIRP

	
GSM/GPRS/EGPRS 900
	TX(Uplink):880M‐915MHZ;

RX(Downlink):925M‐960MHZ
	
34.00 dBm

	
GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M‐1785MHZ;

RX(Downlink):1805M‐1880MHZ
	
29.00 dBm

	
WCDMA B I
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
23.00 dBm

	
WCDMA B VIII
	TX(Uplink): 880-915MHz;

RX(Downlink):925-960MHz
	
24.00 dBm

	
LTE FDD B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
25.00 dBm

	
LTE FDD B3
	TX(Uplink) :1710-1785MHz;

RX(Downlink):1805-1880MHz
	
25.00 dBm

	
LTE FDD B7
	TX(Uplink) :2500-2570MHz;

RX(Downlink):2620-2690MHz
	
25.00 dBm

	
LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz

RX(Downlink): 925 MHz to 960 MHz
	
25.00 dBm

	
LTE FDD B20
	TX(Uplink): 832MHz~862MHz;

RX(Downlink):791MHz~821MHz
	
25.00 dBm

	
LTE FDD B28
	TX(Uplink):    703 MHz to 748MHz

RX(Downlink): 758 MHz to 803 MHz
	
25.00 dBm

	LTE TDD B40
	Uplink & Downlink: 2300 MHz to 2400 MHz
	25.00 dBm

	NFC
	13.56MHz
	32.68dBμA/m@3m

	FM
	Rx(Downlink): 87.5MHz~108MHz
	--

	GPS
	Rx(Downlink): 1575.42MHz
	--




Tests for SAR are conducted using standard operating positions with the device transmitting at its highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body (at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg)

Limitis 2.0(W/kg) for10-g
	10-gHead
	0.662

	
	10-gBody
	0.896

	Limitis 4.0(W/kg) for10-g
	10-gMemberDAS
	1.526






Technical file held by Manufacturer: Shenzhen Gotron Electronic CO.,LTD.
7B01, Building A, Block 1, Anhongji Tianyao Plaza, Longhua District, Shenzhen City, Guangdong Province China

Signed for and on behalf of:                            Shenzhen Gotron Electronic CO.,LTD.

	Name and Title:
	Bing Tang/Manager

	Address:
	7B01, Building A, Block 1, Anhongji Tianyao Plaza, Longhua District, Shenzhen

City, Guangdong Province China






Signature of Authorized Person
2025-06-06
image1.png




image2.png





 


Decla


r


ation of 


C


onformi


t


y (DoC)


 


 


 


We,


 


Shenzhen Gotron Electronic CO.,LTD.


 


7B01, Building A, Block 1, Anhongji Tianyao Plaza, Longhua District, Shenzhen City, Guangdong 


Province China


 


Declare


 


that


 


t


h


e


 


DoC


 


is


 


issued


 


u


n


der


 


o


u


r


 


s


ole


 


r


esponsi


b


il


it


y


 


a


nd


 


b


e


l


o


n


gs


 


to


 


the


 


f


o


l


l


o


w


ing


 


prod


u


ct(s):


 


 


Pro


d


uct


 


T


y


pe:


 


Smart Phone


 


Trademark


：


 


ulefone


 


Model


 


Number(s):


 


GQ5013TF


,


 


Armor 30, Armor 30 Ultra, Armor 30T Ultra, Armor 30T Pro, 


Armor


 


30 Lite, Armor 


30s, Armor 30s Pro


 


 


 


S


y


stem


 


compo


n


ents:


 


 


PIFA


 


Antenna


:


 


B


T/W


i


-


Fi2.4G:


 


-


0.6


 


dBi;


 


WIFI5


.2


G


:


 


1.5 dBi


;


 


WIFI5.8


G


:


 


0.3 dBi


 


GSM900: 


-


2.1dBi


   


PCS1800: 


-


0.74dBi


;


 


WCDMA B


and


 


I: 


0.8 dBi


 


WCDMA B


and


 


VII


I


: 


-


2.1 dBi


;


 


 


L


TE:


 


Band 1: 


0.8 dBi


, Band 3: 


-


0.74


 


dBi, Band 7: 


-


0.35


 


dBi, Band 8: 


-


2.1


 


dBi


,


 


Band 20: 


-


3.4


 


dBi, Band 28: 


-


4.4


 


dBi, 


 


Band 40: 


-


4.38


 


dBi


;


 


 


NFC:


 


Loop Antenna


 


G


PS:


 


PIFA


 


antenna


 


 


Adapter:


 


Model: HJ


-


PD66W


-


EU


 


Input: 100


-


240V AC50/60Hz 1.5A


 


Output: 5.0V


?


3.0A or 9.0V


?


3.0A or 12.0V


?


3.0A


 


or 15.0V


?


3.0A or 20.0V


?


3.25A or 11.0V


?


6.0A 66W MAX


 


 


Manufacturer


 


of the 


adapter:


 


Guangdong Quanzhi Technology Co.,Ltd.


 


 


Rechargeable Li


-


ion Battery:


 


Model:


 


50


13


;


 


Sp


e


cifica


t


ion:


 


D


C


 


3.87


V


,


 


12800


mAh,


 


49.536


Wh


 


 


Manufacturer


 


of 


battery


:


 


Shenzhen Huatiantong Technology Co., Ltd.


 


USB


 


Cable:


 


100


c


m;


 


 


 


 


 




  Decla r ation of  C onformi t y (DoC)       We,   Shenzhen Gotron Electronic CO.,LTD.   7B01, Building A, Block 1, Anhongji Tianyao Plaza, Longhua District, Shenzhen City, Guangdong  Province China   Declare   that   t h e   DoC   is   issued   u n der   o u r   s ole   r esponsi b il it y   a nd   b e l o n gs   to   the   f o l l o w ing   prod u ct(s):    

Pro d uct   T y pe:  Smart Phone  

Trademark ：  ulefone  

Model   Number(s):  GQ5013TF ,   Armor 30, Armor 30 Ultra, Armor 30T Ultra, Armor 30T Pro,  Armor   30 Lite, Armor  30s, Armor 30s Pro  

    S y stem   compo n ents:     PIFA   Antenna :   B T/W i - Fi2.4G:   - 0.6   dBi;   WIFI5 .2 G :   1.5 dBi ;   WIFI5.8 G :   0.3 dBi   GSM900:  - 2.1dBi     PCS1800:  - 0.74dBi ;   WCDMA B and   I:  0.8 dBi   WCDMA B and   VII I :  - 2.1 dBi ;     L TE:   Band 1:  0.8 dBi , Band 3:  - 0.74   dBi, Band 7:  - 0.35   dBi, Band 8:  - 2.1   dBi ,   Band 20:  - 3.4   dBi, Band 28:  - 4.4   dBi,    Band 40:  - 4.38   dBi ;     NFC:   Loop Antenna   G PS:   PIFA   antenna     Adapter:   Model: HJ - PD66W - EU   Input: 100 - 240V AC50/60Hz 1.5A   Output: 5.0V ? 3.0A or 9.0V ? 3.0A or 12.0V ? 3.0A   or 15.0V ? 3.0A or 20.0V ? 3.25A or 11.0V ? 6.0A 66W MAX     Manufacturer   of the  adapter:   Guangdong Quanzhi Technology Co.,Ltd.     Rechargeable Li - ion Battery:   Model:   50 13 ;   Sp e cifica t ion:   D C   3.87 V ,   12800 mAh,   49.536 Wh     Manufacturer   of  battery :   Shenzhen Huatiantong Technology Co., Ltd.   USB   Cable:   100 c m;          

